;; # config for 2.4g
;; normal[Default]: 1~14, 3~11
;; remove FCC: 1~11, 3~9, remove 20M bandwidth channel 12/13/14 and 40M bandwidth 10/11 for special customer requirement.
;; RemoveFCC --> flag = 0: means default setup

[RemoveFCC]
flag = 0